<?xml version="1.0"?>

<SfdcConfigData xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xsd="http://www.w3.org/2001/XMLSchema">

<Modified>true</Modified>

<RoomName>Unnamed Room</RoomName>

<RoomGuid/>

<OccTimeout>1800</OccTimeout>

<DisplayType>Sharp1</DisplayType>

<UseDmRmc>false</UseDmRmc>

<ExternalVideoSwitchIpHostname>Hostname</ExternalVideoSwitchIpHostname>

</SfdcConfigData>

**RoomName** – Fusion Room name, not the device hostname

**DisplayType** – from list below

* Sharp1 (all Sharp displays other than those below)
* Sharp2 (PN-Exx2, PN-Rxx3, PN-Exx3, where “xx” is the screen size)
* Sharp3 (LC-60E77UN, LC-60E88UN)
* Nec1 (Exx3, where “xx” is the screen size)
* Nec2 (Xxx2, where “xx” is the screen size)
* Nec3 (Exx4, where “xx” is the screen size)
* Nec4 (Exx5, where “xx” is the screen size)
* Lg1 (42LG70, 60PA550, 47LN5400)
* Samsung1 (All Samsung UN displays)
* Samsung2 (ME32C)
* Panasonic1 (All Panasonic displays)

**UseDmRmc** – “true” or “false” (without quotes) only. True for a room that will use a DM-RMC-4K-100-C to extend the video to the display in the room. This only applies to the rooms using a DMPS3-4K-150-C.

**ExternalVideoSwitchIpHostname** - IP address in (xxx.xxx.xxx.xxx format) or hostname for the HD-MD4X1-4K-E video switch. Hostname convention should follow format specified by Salesforce.com.

The rest of the text should not be changed in any way.

The file can be called anything, but the extension must be “.dat”

The file must be loaded to the processor in the \User\ folder. This can be done via ftp or toolbox file manager.

There must only by (1) \*.dat file in the \User\ folder. Delete anything already there when making changes or uploading a new file.